Ena

Conf t

Line console 0

Pass ccna@console

Login

Exit

Line vty 0 4

Pass ccna@vty

Login

Exit

Ena secret ccna@enable

Hostname NHANH1

Banner motd #UTTACAD-LAN1-loopback3#

Int g0/0

Desc Connect to LAN1

Ip add 122.0.0.1 255.255.254.0

No shut

Exit

Int s0/0/0

Desc Connect to WAN1

Ip add 122.0.3.129 255.255.255.252

Ipv add 2021:cafe::1/64

No shut

Exit

Int loopback3

Ip add 122.0.3.136 255.255.255.252

No shut

Exit

Ena

Conf t

Line console 0

Pass ccna@console

Login

Exit

Line vty 0 4

Pass ccna@vty

Login

Exit

Ena secret ccna@enable

Hostname NHANH2

Banner motd #UTTACAD–LAN2–LAN3#

Int g0/0

Desc Connect to LAN2

Ip add 122.0.2.1 255.255.255.0

No shut

Exit

Int g0/1

Desc Connect to LAN3

Ip add 122.0.3.1 255.255.255.128

Ipv add 2021::1/64

No shut

Exit

Int s0/1/0

Desc Connect to WAN2

Int add 122.0.3.133 255.255.255.252

Ipv add 2020:2021::1/64

No shut

Exit

Ena

Conf t

Line console 0

Pass ccna@console

Login

Exit

Line vty 0 4

Pass ccna@vty

Login

Exit

Ena secret ccna@enable

Hostname HOME

Banner motd #UTTACAD-Internet#

Int s0/0/0

Ip add 122.0.3.130 255.255.255.252

Ipv add 2021:cafe::2/64

No shut

Exit

Int s0/1/0

Ipv add 122.0.3.134 255.255.255.252

Ipv add 2020:2021::2/64

No shut exit